# Addendum for concession **JAJR180711-149**:

This version of the Otoport Flexi (v3.27.1.46) allows users to vary the acoustic noise reject level during test in 1dB steps.

Therefore, the sections 8.2.5 and 9.2.6 of the user manual which reads:

…

The letter below the indicator represents the noise reject threshold level.

…

Is not representative of the product and should now read:

The number below the indicator indicates the noise reject threshold level in dBSPL.